|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Description** | **Type** | **Value** |
| **commMoveBackward** | Command to move robot backward | Number | 0x02 |
| **commMoveForward** | Command to move robot forward | Number | 0x01 |
| **commStop** | Command to stop robot | Number | 0x00 |
| **commTurnLeft** | Command to turn robot left | Number | 0x03 |
| **commTurnRight** | Command to turn robot right | Number | 0x04 |
| **errBadCommand** | Error: Unknown command received | Number | 0xFF02 |
| **errBadSignal** | Error: Low or Poor signal strength from device | Number | 0xFF01 |
| **errBatteryLow** | Error: Low Battery warning | Number | 0xFF03 |
| **productName** | Name of the physical product | String | “Roboball” |
| **versionNumber** | SDK Version Number | Number | 1.6 |

const commMoveBackward = 0x02;

Command to move robot backward

const commMoveForward = 0x01;

Command to move robot forward

const commStop = 0x00;

Command to stop robot

const commTurnLeft = 0x03;

Command to turn robot left

const commTurnRight = 0x04;

Command to turn robot right

const errBadCommand = 0xFF02;

Error: Unknown command received

const errBadSignal = 0xFF01;

Error: Low or Poor signal strength from device

const errBatteryLow = 0xFF03;

Error: Low Battery warning

const productName = "RoboBall";

Name of the physical product

const versionNumber = 1.6;

SDK Version Number